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[bookmark: Parauga_modeļu_prasības]Sample model requirements
1. [bookmark: 1._Prasības_modeļiem_oriģinālā_formātā:]Requirements for models in original format:
Sample models shall be created in authoring programmes that will be used when performing design work in accordance with the information presented in item 3.6  "Software provision" of the Pre-Contract BIM Execution Plan (including in the presented version of the authoring programme).
Each construction design part manager needs to ensure the development of prototypes, which consists of the following:
· Axis network A-B/1-2. The intersection of the axes A/1 shall be located at the coordinates X;Y;Z=500;500;0. Axis step – 1500 mm in the direction of the X axis and 1250 mm in the direction of the Y axis;
· Spatial figures created with the mass element tool or an analogue. The dimensions of the cube are 1500(x)x1250(y)x1750(z)mm. The height mark of the spatial figure Z= 750 mm and the geometry of the spatial figure in the top view shall coincide with the axis network;
· A data set named “RIX-DATA”* needs to be added to the spatial figure and the following parameters shall be specified in it:
	Attribute
	Explanation

	01 Project discipline
	Specify the parts of the construction design for which the construction design part manager will be responsible

	02 Project manager
	Specify the manager of the part of the construction design

	03 Date
	Specify the date the model was created

	04 Software
	Specify information about the copyright programme


[bookmark: 2._Prasības_modeļiem_*.IFC_failu_formātā]*In some authoring programmes, it is acceptable not to specify the dataset name for technical reasons, but they shall appear in *.IFC file format.
2. Requirements for models in *.IFC file format
It is necessary to export the sample models from the authoring programmes to the *.IFC file format without losing the geometry of the elements and the information specified in item 1. "Requirements for sample models"
Note. In some authoring programmes, it is not possible to export a axis network to *.IFC file format. For the sample models of these author programmes, the lack of an axis network will not be considered as non-compliance with the set requirements.
	

	
3. [bookmark: 3._Prasības_savietotajam_modelim]Requirements for the compatible model
All the created *.IFC templates shall be combined into a single compatible template and it is necessary to make sure that their locations match and that all the information added to the templates is visible.
4. [bookmark: 4._Iesniedzamie_nodevumi]Deliverables
[bookmark: OLE_LINK11]The development of sample models is ensured by the managers of the parts of the construction design specified in item 3.1 of the Pre-Contract BIM Execution Plan. The number of sample models shall match the number of managers of parts of the construction design specified in item 3.1 of the Pre-Contract BIM Execution Plan.
When submitting a proposal during the procurement proposal, the supplier shall submit the following files:

	Deliverable
	Description
	Who provides

	Sample models in original format
	The models developed in the authoring programme containing the 
information specified in item 1
	Managers of parts of the construction design

	Sample models
*.IFC file format
	Models exported from the authoring programme
*.IFC file format without losing its location, geometry and added information
	Managers of parts of the construction design

	The compatible model
	A model that contains information about all sample models, their location, geometry, and added information
	Supplier's BIM Coordinator



