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APPROVED
Procurement Commission of the State Border Guard
Meeting of February 24, 2025
(Meeting Minutes No. 5 of the Procurement Commission, February 24, 2025)

AMENDMENTS TO THE OPEN TENDER
"Procurement of Unmanned Aerial Vehicles for the Needs of the State Border Guard and FRONTEX"
(Procurement Identification Number: VRS 2024/27-01-GP-IDF)
REGULATIONS

The following amendments are made to the regulations of the open tender "Procurement of Unmanned Aerial Vehicles for the Needs of the State Border Guard and FRONTEX" (Procurement Identification Number: VRS 2024/27-01-GP-IDF), which were approved at the meeting of the Procurement Commission of the State Border Guard on February 5, 2025 (Meeting Minutes No. 4 of the Procurement Commission, February 5, 2025):

1. Amend Clause 6.4 of the Regulations as follows:
"6.4. The bidder, within the last three years (i.e., in 2022, 2023, 2024, and until the submission deadline in 2025), has successfully completed at least two contracts similar to the subject of procurement, without any significant violations of the contract or regulatory requirements."

2. Amend the note in Clause 7.2 of the Regulations as follows:

"Note: If the bidder chooses to submit an ESPD, they must also submit an ESPD for each entity whose resources they rely on, as well as for each subcontractor whose service value is at least 10,000 euros. If the bidder is a consortium and chooses to submit an ESPD, each member of the consortium must prepare a separate ESPD for themselves.
3. Delete the note in Clause 14 of the Regulations.

4. Amend Clause 18 of the Regulations as follows:

“When determining the most economically advantageous offer, the contracting authority will consider the following criteria as specified in the table:

	Criteria No.
	Criteria
	Maximum Points

	1.
	Total price of the proposed UAV system, which includes both the product and service costs.
	70

	

	2.
	UAV system aircraft:
	

	2.1.
	Flight duration exceeding 10 hours
	6

	2.2.
	Operating range exceeding 80 km
	5

	2.3.
	Operating temperature range:
	

	2.3.1.
	For temperatures lower than -20°C
	4

	2.3.2.
	For temperatures higher than +35°C
	4

	2.4.
	Maximum flight altitude above sea level (MSL) exceeding 3000m
	3

	2.5.
	Maximum takeoff altitude above sea level (MSL) exceeding 1000m
	3

	2.6.
	Operational capability in windy conditions exceeding 14 m/s
	1

	

	3.
	The power supply must ensure the continuous operation of the GCS and the portable flight path tracking antenna during the UAV flight:
	

	3.1.
	With a portable power station
	4

	3.2.
	With a fuel-powered generator
	2



For criterion 1, the bidder offering the lowest total price will receive the maximum points. Other bidders will be evaluated using the following formula:

P=(X/Y)×Z where: 
P - Calculated score
X - Lowest total offered price 
Y - Evaluated total offered price 
Z - Maximum points available for the criterion.

Evaluation of Criterion 2.1:

Flight Duration 16 hours → 6 points
Flight Duration 15 hours → 5 points
Flight Duration 14 hours → 4 points
Flight Duration 13 hours → 3 points
Flight Duration 12 hours → 2 points
Flight Duration 11 hours → 1 point
Flight Duration 10 hours → 0 points.

Evaluation of Criterion 2.2:

Operating Range 130 km → 5 points
Operating Range 120 km → 4 points
Operating Range 110 km → 3 points
Operating Range 100 km → 2 points
Operating Range 90 km → 1 point
Operating Range 80 km → 0 points.

Evaluation of Criterion 2.3.1:

Lower Temperature Threshold Below -28°C → 4 points

Lower Temperature Threshold Below -26°C → 3 points

Lower Temperature Threshold Below -24°C → 2 points

Lower Temperature Threshold Below -22°C → 1 point

Lower Temperature Threshold -20°C → 0 points.

Evaluation of Criterion 2.3.2:

Higher Temperature Threshold Above +43°C → 4 points

Higher Temperature Threshold Above +41°C → 3 points

Higher Temperature Threshold Above +39°C → 2 points

Higher Temperature Threshold Above +37°C → 1 point

Higher Temperature Threshold +35°C → 0 points.

Evaluation of Criterion 2.4:

Maximum Flight Altitude Above Sea Level (MSL) 6000 m → 3 points

Maximum Flight Altitude Above Sea Level (MSL) 5000 m → 2 points

Maximum Flight Altitude Above Sea Level (MSL) 4000 m → 1 point

Maximum Flight Altitude Above Sea Level (MSL) 3000 m → 0 points.

Evaluation of Criterion 2.5:

Maximum Takeoff Altitude Above Sea Level (MSL) 4000 m → 3 points

Maximum Takeoff Altitude Above Sea Level (MSL) 3000 m → 2 points

Maximum Takeoff Altitude Above Sea Level (MSL) 2000 m → 1 point

Maximum Takeoff Altitude Above Sea Level (MSL) 1000 m → 0 points.

Evaluation of Criterion 2.6, The bidder who meets the wind resistance requirement (above 14 m/s) will receive the allocated points. If the requirement is not met, 0 points will be awarded.
Evaluation of Criterion 3.1, The client awards the specified number of points to the applicant who offers to meet the respective criterion. The applicant who does not offer to meet the respective criterion is assigned a score of "0" for that criterion.

Evaluation of Criterion 3.2, The client awards the specified number of points to the applicant who offers to meet the respective criterion. The applicant who does not offer to meet the respective criterion is assigned a score of "0" for that criterion.


If multiple bids receive the same total score, the bid with the highest score for the offered price will be selected.”

5.
The procurement regulation Annex 2 (Contract for UAV Procurement for the State Border Guard and FRONTEX) Clause 4.12 is amended with the following requirement:

“4.12. [Compliance with Article 62 of the Public Procurement Law is required if the contractor replaces a subcontractor and/or personnel involved in contract execution, or engages a new subcontractor and/or personnel (if applicable)].”
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