

	


Technical specification
Open tender "Maintenance and repair of the Agusta Bell 206B helicopter engine (4 years)"
(Identification No VRS 2024/33-01-ASOP)
1. Definitions
Helicopter – Helicopter “Agusta Bell 206B”.

Helicopter engine — Helicopter`s engine ‘Rolls-Royce 250-C20B’ or component of that engine.

Works – Planned works and Unplanned works.
Planned works — Helicopter engine maintenance and repair works, identified in point 3 “Planned works” of the technical specification as forming part of the planned works.
Unplanned works — Helicopter engine maintenance and repair works, identified in point 4 “Unscheduled works” of the technical specification as forming part of unplanned works.
General Agreement – General Agreement on Works of the Helicopter engine for a period of 4 years from the date of conclusion.

CR - Commission Regulation (EU) No 1321/2014 of 26 November 2014 on the continuing airworthiness of aircraft and aeronautical products, parts and appliances, and on the approval of organisations and personnel involved in these tasks.
LBG – Aviation technical base at the Contracting authority’s disposal in Jaunsmilgas, Isnauda parish, Ludza municipality (main place of activity).
2. General requirements
2.1. Purpose and end result of the service: Perform Planned and Unplanned Works in accordance with the Helicopter Engine Manufacturer's Maintenance Documentation and in accordance with the requirements of the CR;
2.2. Planned and unplanned works are carried out in accordance with aviation industry standards and good practices.
3. Planned works
3.1. At the request of the contracting authority, to carry out the expected maintenance works referred to in the table of this technical specification on Planned works on the engine (hereinafter – Table). 
3.2. The final result of the works: Helicopter engine re-airworthiness or re-resource according to Contracting authority 's request. 
3.3. Quality requirements for planned works, resources and methods to be used:
3.3.1. Planned works are carried out at the places of work mentioned in Table. 
3.3.2. The Contracting authority dismantles/assemblies, packs and pays for delivery services for the transfer of the Helicopter engine to the place of work at his own expense.
3.3.3. After completion of the Planned Works, the Contractor sends the Helicopter engine to LBG and pays for courier services (Incoterms 2020, DAP) for the transfer of the component from the repair site.
3.3.4. Planned works are carried out using the resources available to the Contractor: raw materials, spare parts, special equipment and keys. 
List of planned works of the helicopter engine during the period of validity of the General Agreement:
	Nr.p.k.
	Name of the planned work
	Planned work order year by planned flight hours
	Unit of measurement
	Quantity

	1.
	Engine turbine Heavy maintenance inspection (HMI) p/n 23069745 
	2028 – 2029
	pcs.
	1

	2.
	Engine Gas producer turbine p/n M250-10223 1st Stage Wheel replacement
	2028 – 2029
	pcs.
	1

	3.
	Engine Gas producer turbine p/n 230073854 2.nd Stage Wheel replacement
	2028 – 2029
	pcs.
	1

	4.
	CEB A-1370 Engine, Turbine- Inspection Of 1st Stage Nozzle Shield Dome 
	2028 – 2029
	pcs.
	1

	5.
	CEB A-1375 Engine, Turbine- Replacement Of 2st Stage Nozzle Diaphragm 
	2028 – 2029
	pcs.
	1


Note: 2025-2027 Planned works of the helicopter engine based on planned annual flying hours and technical documentation of the manufacturer of the helicopter engine are not planned.
4. Unplanned works
4.1. Purpose and end result of the service: to carry out helicopter maintenance works and repairs which are not part of the Scheduled Works and which need to be carried out in order to restore the airworthiness or resource of the helicopter engine after the Contracting authority has detected defects or damage to the helicopter that prevent the helicopter from starting the flight, as well as unexpected maintenance works and repairswhich the Contractor detects only during the performance of the Works and which cannot be detected without dismantling the helicopter engine. 
4.2. The final result of theworks: Helicopter engine re-airworthiness or re-resource in accordance with the Contracting authority 's request. 
4.3. Quality requirements, resources and methods to be used for unplanned works:
4.3.1. Unplanned works shall be carried out at the place of performance of the works requested in accordance with the procedures laid down in the General Agreement;
4.3.2. If the workplace of Unplanned works is LBG, then the Contractor authority shall, by separate request, request the presence of the Contractor's certified personnel for the time of performing the Unplanned Works at the LBG.
4.3.3. If the workplace is not LBG, then the Contracting authority dismantles/assemblies, packs and pays for delivery services for the transfer of the Helicopter engine to the place of work;
4.3.4. After completion of the unplanned works, the Contractor shall, in accordance with the Contracting authority 's request:
4.3.4.1. sends the Helicopter engine to LBG and pays for courier services (Incoterms 2020, DAP) for the transfer of the Helicopter engine from the place of repair or;
4.3.4.2. transfer the Helicopter engine to the courier using the Contracting authority 's Client Number (Incoterms 2020, Ex Works)to transfer the Helicopter engine to LBG.
4.3.5. Unplanned works are carried out using the resources at the disposal of the Contractor: raw materials, spare parts, special equipment and keys (all shall be included in the price of unscheduled work, except for the special equipment and spare parts referred to in Clause 5, if unscheduled work is requested by LBG). Before starting unplanned works, the Contracting authority and the Contractor agree what spare parts will be used in the respective repair (the Contracting authority (from existing stocks) or/and the Contractor ensures (delives) the execution of unplanned works with raw materials and spare parts). 
5. Use of special equipment and special keys
The Contractor uses special equipment and special keys at the Contracting authority 's disposal to perform unplanned work that can be performed by LBG. If the Contracting authority does not have the necessary special equipment or a special key at his disposal, the Contractor shall use the special equipment and special keys at his disposal, which are necessary for the performance of the Works.
